|  |  |  |  |
| --- | --- | --- | --- |
|  | Topic | Page | Include? |
| A | Introduction | 10 |  |
| B | Integrated Clinical Environment (ICE) Clinical Scenarios | 11 |  |
| UC.1 | ICE.1 - Safety Interlocks | 11 |  |
| UC.2 | ICE.2 - Synchronization with safety interlock | 12 |  |
| UC.3 | ICE.3 - Process control (workflow) | 14 |  |
| UC.4 | ICE.4 - Smart alarm system | 14 |  |
| UC.5 | ICE.5 - Decision support | 15 |  |
| UC.6 | ICE.6 - Physiological Closed Loop Control (PCLC) | 17 |  |
| UC.7 | ICE.7 - Medical Device Plug-and-Play Interoperability (MD PnP) | 18 |  |
| C | SDC/QH – Quiet Hospital (QH) Scenario and Use Cases | 20 |  |
| UC.8 | SDC/QH.1 – Device alert signal delegation to single-pt. alert aggregator | 20 |  |
| UC.9 | SDC/QH.2 – Single pt. alert aggregator alert signal delegation to multi-pt. aggregator | 21 |  |
| UC.10 | SDC/QH.3 – Device alert signal delegation to Alert Manager (ACM AM) | 21 |  |
| UC.11 | SDC/QH.4 – Multi-pt. aggregator to Alert Manager (ACM AM) | 21 |  |
| UC.12 | SDC/QH.5 – SDC to FHIR® Gateway. | 21 |  |
| UC.13 | SDC/QH.6 – Alert Manager (ACM AM) to care-giver Alert Communicator (ACM AC) | 21 |  |
| UC.14 | SDC/QH.7 – Alert Communicator (ACM AC) failure | 21 |  |
| UC.15 | SDC/QH.8 – Alert Manager (ACM AM) failure | 21 |  |
| UC.16 | SDC/QH.9 – Multi-pt. aggregator failure | 22 |  |
| UC.17 | SDC/QH.10 – Single pt. aggregator failure | 22 |  |
| D | SDC/PDP - Preeclampsia (PDP) Scenario and Use Cases | 23 |  |
| UC.18 | SDC/PDP.1 - In-hospital, at home and mobile / clinic care contexts | 23 |  |
| UC.19 | SDC/PDP.2 - Acute point-of-care medical and personal health devices | 23 |  |
| UC.20 | SDC/PDP.3 - Lab results including point of care devices and transactions | 23 |  |
| UC.21 | SDC/PDP.4 - Location tracking and Device Identification / Association Management | 23 |  |
| UC.22 | SDC/PDP.5 - A Cloud-based CDS system and “locally” networked systems & applications | 24 |  |
| E | SDC/FESS – Endoscopic Surgery Scenario and Use Cases | 25 |  |
| UC.23 | SDC/FESS.1 – Surgeon view of patient vitals | 25 |  |
| UC.24 | SDC/FESS.2– Surgeon control of OR table and lights | 25 |  |
| UC.25 | SDC/FESS.3– Surgeon control of surgical tools | 25 |  |
| UC.26 | SDC/FESS.4 – Device reports technical issue to responsible BMET | 26 |  |
| UC.27 | SDC/FESS.5 – Seamless exchange of Medical Devices | 26 |  |
| F | NITRD – Medical Device Scenario and Use Cases | 27 |  |
| UC.28 | NITRD.1 – Seamless changes of medical devices | 28 |  |
| UC.29 | NITRD.2 – Capture of data and settings | 28 |  |
| UC.30 | NITRD.3 – Supervisory control established | 28 |  |
| UC.31 | NITRD.4 – Autonomous patient therapy | 28 |  |
| UC.32 | NITRD.5 – Data flows through the Continuum of Care | 28 |  |
| UC.33 | NITRD.6 – Capture of equipment configurations | 28 |  |
| UC.34 | NITRD.7 – Black Box Recorder | 28 |  |
| G | OR.NET Use Cases | 29 |  |
| UC.35 | ORNET.001 - Integration of anesthesia video data into (anesthesiologic) patient monitoring via radio transmission | 29 |  |
| UC.36 | ORNET.004 - Indicates a warning from one OSCB-compliant device to another | 29 |  |
| UC.37 | ORNET.005 - Transfer of the control of device A by a device B, which is actually prohibited | 29 |  |
| UC.38 | ORNET.006 - User-specific workflow-dependent adjustment of the height of the operating table / foot step | 29 |  |
| UC.39 | ORNET.009 - Display of electrophysiological signals on a monitor by a surgeon | 29 |  |
| UC.40 | ORNET.010 - Use of a foot switch as an input device | 29 |  |
| UC.41 | ORNET.012 - Display of force and moment sensor (KMS) for knee axis determination on central monitor | 29 |  |
| UC.42 | ORNET.016 - Collision avoidance of devices | 29 |  |
| UC.43 | ORNET.017 - Control of a desired manipulator by a common control console | 29 |  |
| UC.44 | ORNET.018 - Power control of the milling machine at the middle | 29 |  |
| UC.45 | ORNET.019 - Linking the surgical light to the endoscope | 29 |  |
| UC.46 | ORNET.024 - Storage of intraoperative image data in the EHR | 29 |  |
| UC.47 | ORNET.029 - Intraoperative input of monitoring data to EHR | 29 |  |
| UC.48 | ORNET.030 - Display of monitoring data in microscope image | 29 |  |
| UC.49 | ORNET.032 - Insertion of relevant information into the surgical microscope according to the clinical situation | 29 |  |
| UC.50 | ORNET.035 - Central presentation of relevant device data / documents / patient data close to the site | 29 |  |
| UC.51 | ORNET.040 - Single check-desk | 30 |  |
| UC.52 | ORNET.042 - prevention of explosions | 30 |  |
| UC.53 | ORNET.043 - Controlling the US Dissector with the Human Machine Interface (MMI) of the microscope | 30 |  |
| UC.54 | ORNET.050 - Service Total Log | 30 |  |
| UC.55 | ORNET.051 - Visualization of instrument position | 30 |  |
| UC.56 | ORNET.051 - Visualization of instrument position | 30 |  |
| UC.57 | ORNET.067 - Fusion imaging intraoperatively US - CT / MRT | 30 |  |
| UC.58 | ORNET.068 - Image-based communication. | 30 |  |
| UC.59 | ORNET.069 - Monitoring of patient and device parameters, especially alarms | 30 |  |
| UC.60 | ORNET.070 - Control of the anesthesiologically relevant device parameters. | 30 |  |
| UC.61 | ORNET.072 - Import of clinical data from the EHR | 30 |  |
| UC.62 | ORNET.073 - Storage of digital patient records in the EHR. | 30 |  |
| UC.63 | ORNET.078 - Operating room preparation | 30 |  |
| UC.64 | ORNET.079 - remote diagnostics remote maintenance firmware update | 30 |  |
| UC.65 | ORNET.082 - Video display of selected parameters from external OSCB-compliant devices | 30 |  |
| UC.66 | ORNET.084 - Transfer of a 3D volume image to a navigation system | 30 |  |
| UC.67 | ORNET.086 - Storing an Endoscope Video | 30 |  |
| UC.68 | ORNET.090 - Position adjustment C-arm and operating table | 30 |  |
| UC.69 | ORNET.091 - Insertion of tumor borders into the microscope. | 30 |  |
| UC.70 | ORNET.095 - Control of the endoscope light source via the navigation MMI | 30 |  |
| UC.71 | ORNET.096 - Integration of B-Mode ultrasound into navigation | 30 |  |
| UC.72 | ORNET.097 - Integration of 3D ultrasound into navigation. | 31 |  |
| UC.73 | ORNET.100 - uploading patient strain data to the medical IT subnet | 31 |  |
| UC.74 | ORNET.101 - Coupling of the footing height to the seat height | 31 |  |
| UC.75 | ORNET.102 - Detection of OSCB compliant devices | 31 |  |
| UC.76 | ORNET.103 - Failure of OSCB compliant devices | 31 |  |
| UC.77 | ORNET.104 - Logout of OSCB-compliant devices | 31 |  |
| UC.78 | ORNET.105 - Automatic feeding of patient strain data to OSCB compliant device | 31 |  |
| UC.79 | ORNET.106 - Enter the operator ID in the IT subnet | 31 |  |
| UC.80 | ORNET.107 - Automatic input of operator code in OSCB-compliant device. | 31 |  |
| UC.81 | ORNET.108 - Transfer of image data from the PACS to a monitor | 31 |  |
| UC.82 | ORNET.109 - Create intraoperative screenshots. | 31 |  |
| UC.83 | ORNET.110 - Transfer registration information from the navigation device to the robotic system | 31 |  |
| UC.84 | ORNET.111 - Display additional information on the monitor of the navigation device | 31 |  |
| UC.85 | ORNET.112 - Load planning image data from the PACS into the robotic system | 31 |  |
| UC.86 | ORNET.114 - Recording and archiving of video data for documentation via a Frame grabber application | 31 |  |
| UC.87 | ORNET.115 - Recording and archiving of video data for documentation via an IP data stream | 31 |  |
| UC.88 | ORNET.116 - View of DICOM® objects on any terminal with display function | 31 |  |
| UC.89 | ORNET.117 - Patient and surgical centered DICOM object display | 31 |  |
| UC.90 | ORNET.118 - Storage of DICOM objects in DICOM object-recording systems | 32 |  |
| UC.91 | ORNET.119 - Control from a DICOM object viewer to change the layout of a display screen | 32 |  |
| UC.92 | ORNET.120 - Linking the OP light to the C-arm | 32 |  |
| UC.93 | ORNET.121 - Reconstruction of the OP Situs by laser measuring point. | 32 |  |
| UC.94 | ORNET.122 - Power control of the vacuum cleaner on the central pipe. | 32 |  |
| UC.95 | ORNET.123 - Derivation of the alarms of the surgical alarm system to the operating theater | 32 |  |
| UC.96 | ORNET.124 - Alarm-triggered manipulation of the RGB room light | 32 |  |
| UC.97 | ORNET.125 - Show warning signals in videos of minimally / non-invasive imaging procedures | 32 |  |
| UC.98 | ORNET.126 - Re-adjustment of preoperative CT data using intraoperative DVT | 32 |  |
| UC.99 | ORNET.127 - Automatic orientation of the stereo camera | 32 |  |
| UC.100 | ORNET.128 - Logging the Instrument Position During Optical Navigation | 32 |  |
| UC.101 | ORNET.129 - Transfer of a log to the logistics system | 32 |  |
| UC.102 | ORNET.130 - Integration of neuromonitoring of the ENT area into the optical navigation | 32 |  |
| UC.103 | ORNET.131 - Adjust the position of the operating table using a navigated pointer | 32 |  |
| UC.104 | ORNET.132 - Common control interface for all devices. | 32 |  |
| UC.105 | ORNET.133 - Automatic documentation of device parameters: blood volume | 32 |  |
| UC.106 | ORNET.134 - Automatic documentation of device parameters: surface dose. | 32 |  |
| UC.107 | ORNET.135 - Combination of rotational angiography with electrophysiological measuring site | 32 |  |
| UC.108 | ORNET.136 - CT / MRI linkage with TEE ultrasound in endoscopic mitral valve surgery | 32 |  |
| UC.109 | ORNET.137 - Common operation of all room air-conditioning units from sterile workplaces | 33 |  |
| UC.110 | ORNET.138 - Availability of all patients Information from sterile workplace | 33 |  |
| UC.111 | ORNET.139 - Power control of an ultrasonic breaker | 33 |  |
| UC.112 | ORNET.140 - Integration of neuromonitoring of the brain into the risk areas of optical navigation | 33 |  |
| UC.113 | ORNET.141 - Integration of intraoperative ultrasound data of neurosurgery into the risk areas of optical navigation | 33 |  |
| UC.114 | ORNET.142 - Adaptation of device parameters to vital parameters of patient | 33 |  |
| UC.115 | ORNET.143 - Adaptation of device parameters to patient 's vital parameters | 33 |  |
| UC.116 | ORNET.144 - Integration of the Laparoscopy and Endoscopy Tower | 33 |  |
| UC.117 | ORNET.145 - Linking the surgical column and the operating table | 33 |  |
| UC.118 | ORNET.146 - Warning if pressure is too strong on the ultrasound device | 33 |  |
| UC.119 | ORNET.147 - Change the US dissector parameters | 33 |  |
| UC.120 | ORNET.148 - Remote triggering of US dissector device functionalities | 33 |  |
| UC.121 | ORNET.149 - US dissector informs the microscope of its current trigger state | 33 |  |
| UC.122 | ORNET.150 - Remote tripping of US dissector device functionalities | 33 |  |
| UC.123 | ORNET.151 - Acoustic and visual feedback of intraoperative neuromonitoring during surgical procedures | 33 |  |
| UC.124 | ORNET.152 - Transfer of video and image data | 33 |  |
| UC.125 | ORNET.153 - Read image data from the PACS | 33 |  |
| UC.126 | ORNET.154 - Uploading image data to the PACS | 33 |  |
| UC.127 | ORNET.155 - File import from the EHR | 33 |  |
| UC.128 | ORNET.156 - File export to the EHR | 33 |  |
| H | IHE PCD - Device to Enterprise Communication (DEC) Use Cases | 34 |  |
| UC.129 | DEC.1 - Communicate patient identified DEC data to EMR/EHR | 34 |  |
| UC.130 | DEC.2 - Communicate validated periodic DEC data to EMR/EHR | 34 |  |
| UC.131 | DEC.3 - Use Cases for Automatic Patient Demographics Acquisition | 34 |  |
| UC.132 | DEC.3.1 - Patient ID known in ADT, locally available | 35 |  |
| UC.133 | DEC.3.2 - Patient ID known in ADT, not locally available | 35 |  |
| UC.134 | DEC.3.3 - Patient ID not known in ADT, locally available | 35 |  |
| UC.135 | DEC.3.4 - Patient ID not known in ADT, not locally available. | 35 |  |
| UC.136 | DEC.3.5 Other Clinical Examples | 36 |  |
| UC.137 | DEC.3.5a – Association of Patient ID and Medical Device – via ID List | 36 |  |
| UC.138 | DEC.3.5b - Association of Patient ID and Medical Device – via patient wristband | 36 |  |
| UC.139 | DEC.3.5c - Association of Patient ID and Medical Device – via RFID tags | 36 |  |
| I | IHE PCD - DEC Subscribe to Patient Data (SPD) Use Cases | 37 |  |
| UC.140 | SPD.1: Communicate patient identified data to EMR/EHR | 37 |  |
| UC.141 | SPD.2 - Communicate validated periodic data to EMR/EHR | 37 |  |
| UC.142 | SPD.3 - Subscribe to patient data at specific periodic interval. | 37 |  |
| UC.143 | SPD.4 - Subscribe to patient data for specific patients. | 37 |  |
| UC.144 | SPD.5 - Subscribe to patient data for patients from a specific location. | 37 |  |
| UC.145 | SPD.6 - Subscribe to patient data for a specific device or class of devices | 37 |  |
| UC.146 | SPD.7 - Subscribe to patient data for specific parameters or class of parameters. | 38 |  |
| UC.147 | SPD.8 - Request a snapshot of current or most recent patient data. | 38 |  |
| J | IHE PCD - Alert Communication Management (ACM) Use Cases | 39 |  |
| UC.148 | ACM.1 - Location Sourced | 39 |  |
| UC.149 | ACM.2 - Identified Patient Source | 39 |  |
| UC.150 | ACM.3 - Same as ACM.1/ACM.2 with Escalation with Cancel at Alert Source | 40 |  |
| UC.151 | ACM.4 - Same as ACM.1/ACM.2 with Escalation with Cancel at Communication Endpoint | 40 |  |
| UC.152 | ACM.5 - Same as ACM.1/ACM.2 with Escalation with Cancel at AM | 40 |  |
| UC.153 | ACM.6 - Information with no destination other than logging by the AM | 40 |  |
| UC.154 | ACM.7 - Equipment Sourced Alert | 40 |  |
| K | IHE PCD - Medical Equipment Management Device Management (MEMDMC) Use Cases | 41 |  |
| UC.155 | MEMDMC.1 - Equipment Observations to CMMS | 41 |  |
| UC.156 | MEMDMC.2 - Equipment Observations to CMMS | 41 |  |
| L | IHE PCD - Medical Equipment Management Location Services (MEMLS) Use Cases | 43 |  |
| UC.157 | MEMLS.1 - Communication of location observations in conjunction with other non-location related transactions | 43 |  |
| UC.158 | MEMLS.2 - Communication of location observations in conjunction with LS specific events | 43 |  |
| M | IHE PCD - Waveform Content Module (WCM) Use Cases | 45 |  |
| UC.159 | WCM.1 - Alarm Waveform Snapshot | 45 |  |
| UC.160 | WCM.2 - Real-Time Waveform Viewing | 45 |  |
| UC.161 | WCM.3 - Archived Waveform Viewing | 45 |  |
| UC.162 | WCM.4 - Mixed Snapshot and Continuous Waveform Viewing | 45 |  |
| UC.163 | WCM.5 - Waveform Snapshot to EHR | 45 |  |
| UC.164 | WCM.6 - 12 Lead ECG | 45 |  |
| N | IHE PCD - Retrospective Data Query (RDQ) Use Cases | 46 |  |
| UC.165 | RDQ.1 - Query for all retrospective data on a single patient. | 46 |  |
| UC.166 | RDQ.2 - Query for all retrospective data on multiple patients. | 46 |  |
| UC.167 | RDQ.3 - Query for retrospective data on a single patient within a specified time interval. | 47 |  |
| UC.168 | RDQ.4 - Query for retrospective data on multiple patients within a specified time interval. | 47 |  |
| UC.169 | RDQ.5 - Query for retrospective data on 1 or more parameter elements on a single patient. | 47 |  |
| UC.170 | RDQ.6 - Query for retrospective data on 1 or more parameter elements on multiple patients. | 48 |  |
| UC.171 | RDQ.7 - Query for retrospective data on 1 or more parameter elements on a single patient within a specified time interval. | 48 |  |
| UC.172 | RDQ.8 - Query for retrospective data on 1 or more parameter elements on multiple patients within a specified time interval. | 48 |  |
| O | IHE PCD - Implantable Device Cardiac Observation (IDCO) Use Cases | 50 |  |
| UC.173 | IDCO.1 - Implantable Cardiac Device In-Clinic Follow-up | 50 |  |
| UC.174 | IDCO.2 - Implantable Cardiac Device In-Clinic Follow-up with Networked Programmer that Translates Information | 51 |  |
| UC.175 | IDCO.3 - Implantable Cardiac Device Remote Followup | 51 |  |
| UC.176 | IDCO.4 - Remote Monitoring of Implanted Cardiac Devices | 51 |  |
| P | IHE PCD - Point-of-Care Infusion Verification (PIV) Use Cases | 53 |  |
| UC.177 | PIV.1 – Transfer of infusion parameters from BPOC to infusion device | 53 |  |
| Q | IHE PCD - Infusion Pump Event Communication (IPEC) | 55 |  |
| UC.178 | IPEC.1: Communicate event data to EMR/EHR | 55 |  |
| R | IHE PCD - Point-of-Care Identity Management (PCIM) Use Cases | 56 |  |
| UC.179 | PCIM.1 - Associating Device with Patient | 56 |  |
| UC.180 | PCIM.2 - Disassociating Device from Patient | 57 |  |
| UC.181 | PCIM.3 - Query for the Devices for a Patient | 58 |  |
| UC.182 | PCIM.4 - Query the Associated Patient for a Device | 58 |  |
| UC.183 | PCIM.5 - Device Registrant Registers a Device | 58 |  |
| UC.184 | PCIM.6 - Query the Device Registrant for a list of candidate devices for an association | 59 |  |
| S | CEN/TC 251/PT5-021 (VITAL) Use Cases | 60 |  |
| UC.185 | VITAL.1 - Data Logger - Single Device | 62 |  |
| UC.186 | VITAL.2 - Data Logger - Multiple Devices | 64 |  |
| UC.187 | VITAL.3 - Real-Time Data Display | 67 |  |
| UC.188 | VITAL.4 - Patient Alarm Monitoring | 68 |  |
| UC.189 | VITAL.5 - Remote Control | 70 |  |
| UC.190 | VITAL.6 - Patient Viewing Interoperability | 71 |  |
| UC.191 | VITAL.7 - Patient Monitoring Interoperability | 73 |  |
| UC.192 | VITAL.8 - Patient Data Exchange (Off-line) | 74 |  |
| UC.193 | VITAL.9 - Patient Data Exchange (On-line/Interactive) | 76 |  |
| T | ONC/AHIC Common Device Connectivity Use Cases | 79 |  |
| UC.194 | AHIC.1 - Configure and register a device to communicate with an EHR. | 80 |  |
| UC.195 | AHIC.2 - Associate patient ID and device information within an EHR. | 80 |  |
| UC.196 | AHIC.3 - Communicate measurement information to the EHR | 80 |  |
| UC.197 | AHIC.4 - Communicate device meta-data with each measurement to the EHR. | 81 |  |
| UC.198 | AHIC.5 - Communicate measurement intervals, etc. within the EHR. | 81 |  |
| UC.199 | AHIC.6 - Query the device or device intermediary for additional information. | 81 |  |
| UC.200 | AHIC.7 – Gracefully recover from a lapse in EHR connectivity. | 82 |  |
| UC.201 | AHIC.8 - Communicate standardized alarm types to the EHR. | 82 |  |
| UC.202 | AHIC.9 - Set limits and safeguards for device settings from the EHR to a device. | 82 |  |
| UC.203 | AHIC.10 - Wirelessly communicate PoC device information from the device to a device intermediary or EHR. | 82 |  |
| U | “Special” Patient Monitoring Use Cases | 90 |  |
| UC.204 | PM.1 - Synchronized Cardioversion | 90 |  |
| UC.205 | PM.2 - Intra-Aortic Balloon Pump Synchronization | 90 |  |
| UC.206 | PM.3 - Catheter Insertion Procedure | 91 |  |
| UC.207 | PM.4 - The User “Cockpit” | 91 |  |
|  |  |  |  |